(module "NodeMCU1.0(12-E)" (layer F.Cu) (tedit 5AF3DDCB)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value "NodeMCU1.0(12-E)" (at 0 -5.08) (layer F.Fab))
  (fp_text user USB (at 0 22.86) (layer F.SilkS))
  (fp_text user "RF Antenna" (at 0 -20.32) (layer F.SilkS))
  (fp_text user VIN (at -11.43 17.78) (layer F.SilkS))
  (fp_text user G (at -11.43 15.24) (layer F.SilkS))
  (fp_text user RST (at -11.43 12.7) (layer F.SilkS))
  (fp_text user EN (at -11.43 10.16) (layer F.SilkS))
  (fp_text user 3V (at -11.43 7.62) (layer F.SilkS))
  (fp_text user G (at -11.43 5.08) (layer F.SilkS))
  (fp_text user SK (at -11.43 2.54) (layer F.SilkS))
  (fp_text user SO (at -11.43 0) (layer F.SilkS))
  (fp_text user SC (at -11.43 -2.54) (layer F.SilkS))
  (fp_text user S1 (at -11.43 -5.08) (layer F.SilkS))
  (fp_text user S2 (at -11.43 -7.62) (layer F.SilkS))
  (fp_text user S3 (at -11.43 -10.16) (layer F.SilkS))
  (fp_text user VU (at -11.43 -12.7) (layer F.SilkS))
  (fp_text user G (at -11.43 -15.24) (layer F.SilkS))
  (fp_text user A0 (at -11.43 -17.78) (layer F.SilkS))
  (fp_text user 3V (at 11.43 17.78) (layer F.SilkS))
  (fp_text user G (at 11.43 15.24) (layer F.SilkS))
  (fp_text user TX (at 11.43 12.7) (layer F.SilkS))
  (fp_text user RX (at 11.43 10.16) (layer F.SilkS))
  (fp_text user D8 (at 11.43 7.62) (layer F.SilkS))
  (fp_text user D7 (at 11.43 5.08) (layer F.SilkS))
  (fp_text user D6 (at 11.43 2.54) (layer F.SilkS))
  (fp_text user D5 (at 11.43 0) (layer F.SilkS))
  (fp_text user G (at 11.43 -2.54) (layer F.SilkS))
  (fp_text user 3V (at 11.43 -5.08) (layer F.SilkS))
  (fp_text user D4 (at 11.43 -7.62) (layer F.SilkS))
  (fp_text user D3 (at 11.43 -10.16) (layer F.SilkS))
  (fp_text user D2 (at 11.43 -12.7) (layer F.SilkS))
  (fp_text user D1 (at 11.43 -15.24) (layer F.SilkS))
  (fp_text user D0 (at 11.43 -17.78) (layer F.SilkS))
  (pad 1 thru_hole circle (at -13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at -13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at -13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at -13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at -13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 9 thru_hole circle (at -13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 10 thru_hole circle (at -13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 11 thru_hole circle (at -13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 12 thru_hole circle (at -13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 13 thru_hole circle (at -13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 14 thru_hole circle (at -13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 15 thru_hole circle (at -13.97 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 16 thru_hole circle (at 13.97 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 17 thru_hole circle (at 13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 18 thru_hole circle (at 13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 19 thru_hole circle (at 13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 20 thru_hole circle (at 13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 21 thru_hole circle (at 13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 22 thru_hole circle (at 13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 23 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 24 thru_hole circle (at 13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 25 thru_hole circle (at 13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 26 thru_hole circle (at 13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 27 thru_hole circle (at 13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 28 thru_hole circle (at 13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 29 thru_hole circle (at 13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  (pad 30 thru_hole circle (at 13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
)
