(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "jlpcb/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D2-BA)")
	(net 2 "Net-(D2-GA)")
	(net 3 "GND")
	(net 4 "Net-(D2-RA)")
	(net 5 "VCC")
	(net 6 "Net-(D3-A)")
	(net 7 "NEUT")
	(net 8 "unconnected-(J1-Pin_2-Pad2)")
	(net 9 "/LineRadiateur")
	(net 10 "unconnected-(J2-Pin_2-Pad2)")
	(net 11 "LINE")
	(net 12 "Net-(J5-GCLK0{slash}GPIO4)")
	(net 13 "unconnected-(J5-SCL{slash}GPIO3-Pad5)")
	(net 14 "unconnected-(J5-GPIO15{slash}RXD-Pad10)")
	(net 15 "Net-(J5-GPIO17)")
	(net 16 "unconnected-(J5-GPIO26-Pad37)")
	(net 17 "unconnected-(J5-GPIO27-Pad13)")
	(net 18 "unconnected-(J5-~{CE0}{slash}GPIO8-Pad24)")
	(net 19 "Net-(U2-VDD)")
	(net 20 "unconnected-(J5-3V3-Pad17)")
	(net 21 "Net-(J5-MOSI0{slash}GPIO10)")
	(net 22 "unconnected-(J5-PWM0{slash}GPIO12-Pad32)")
	(net 23 "unconnected-(J5-GPIO19{slash}MISO1-Pad35)")
	(net 24 "Net-(J5-GPIO22)")
	(net 25 "unconnected-(J5-ID_SD{slash}GPIO0-Pad27)")
	(net 26 "unconnected-(J5-GPIO20{slash}MOSI1-Pad38)")
	(net 27 "unconnected-(J5-SCLK0{slash}GPIO11-Pad23)")
	(net 28 "Net-(J5-GPIO23)")
	(net 29 "unconnected-(J5-GPIO14{slash}TXD-Pad8)")
	(net 30 "unconnected-(J5-~{CE1}{slash}GPIO7-Pad26)")
	(net 31 "unconnected-(J5-GPIO21{slash}SCLK1-Pad40)")
	(net 32 "unconnected-(J5-GPIO18{slash}PWM0-Pad12)")
	(net 33 "unconnected-(J5-GCLK1{slash}GPIO5-Pad29)")
	(net 34 "Net-(J5-GPIO16)")
	(net 35 "unconnected-(J5-PWM1{slash}GPIO13-Pad33)")
	(net 36 "unconnected-(J5-GCLK2{slash}GPIO6-Pad31)")
	(net 37 "unconnected-(J5-GPIO25-Pad22)")
	(net 38 "Net-(J5-MISO0{slash}GPIO9)")
	(net 39 "unconnected-(J5-SDA{slash}GPIO2-Pad3)")
	(net 40 "unconnected-(J5-ID_SC{slash}GPIO1-Pad28)")
	(net 41 "Net-(J5-GPIO24)")
	(net 42 "unconnected-(J5-5V-Pad2)")
	(net 43 "Net-(J9-Pin_1)")
	(net 44 "unconnected-(K1-Pad4)")
	(net 45 "Net-(Q1-B)")
	(net 46 "Net-(Q1-C)")
	(net 47 "Net-(Q2-B)")
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 65.5 47)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J5-GPIO17)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(Q1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 75.66 43 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U2-VDD)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J5-GCLK0{slash}GPIO4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm-4_RGB_Wide_Pins"
		(layer "F.Cu")
		(at 65.182 63.5)
		(descr "LED, diameter 5.0mm, 4 pins, WP154A4, https://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.11A).pdf")
		(tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED")
		(property "Reference" "D2"
			(at 6.818 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RGBC"
			(at 3.2385 3.96 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D2-RA)")
			(pinfunction "RA")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.159 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 4.318 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D2-GA)")
			(pinfunction "GA")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 6.477 0)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D2-BA)")
			(pinfunction "BA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB_Wide_Pins.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical"
		(layer "F.Cu")
		(at 136.2425 63.0225 90)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1836299 8A 320V")
		(tags "phoenix_contact connector MCV_01x02_G_5.08mm")
		(property "Reference" "J7"
			(at 2.54 -5.55 90)
			(layer "F.SilkS")
		)
		(property "Value" "230V IN"
			(at -4.4775 -1.2425 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 11 "LINE")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "NEUT")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 65.42 51.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J5-GPIO16)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(Q2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 47 44.5 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.5 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J5-GPIO22)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D2-RA)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 109.275 64 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J8"
			(at -2.2 2.275 180)
			(layer "F.SilkS")
		)
		(property "Value" "5V IN"
			(at 0.4 -3.825 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 100.5 46.46 -90)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 1.04 3 90)
			(layer "F.SilkS")
		)
		(property "Value" "2N2222"
			(at 1.27 2.79 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.unisonic.com.tw/datasheet/S8050.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.7A Ic, 20V Vce, Low Voltage High Current NPN Transistor, TO-92"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 122.5 52.5)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "ToTransfo"
			(at 0 9 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "NEUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(J2-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LINE")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 36.92 39.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.08 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J5-GPIO24)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D2-BA)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 90.5 49 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "27"
			(at 5.08 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(Q1-C)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical"
		(layer "F.Cu")
		(at 136 42 90)
		(descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-5.08; number of pins: 03; pin pitch: 5.08mm; Vertical || order number: 1836309 8A 320V")
		(tags "phoenix_contact connector MCV_01x03_G_5.08mm")
		(property "Reference" "J1"
			(at 5.08 -5.55 90)
			(layer "F.SilkS")
		)
		(property "Value" "Radiateur Out"
			(at 5.08 4.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 7 "NEUT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 10.16 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LineRadiateur")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 44.62 63.5 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "9/10/GND/V+"
			(at 2.5 3.12 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J5-MOSI0{slash}GPIO10)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J5-MISO0{slash}GPIO9)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 100 54.46 -90)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 1.04 2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "PN2222A"
			(at 1.27 2.79 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J9-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 99.5 41.31 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D3"
			(at 3.81 -2.12 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4448"
			(at 3.81 2.12 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A High-speed standard diode, DO-35"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
		(layer "F.Cu")
		(at 106.85 36.45)
		(descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
		(tags "relay Sanyu SRD form C")
		(property "Reference" "K1"
			(at 8.1 9.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "5V Relais / coil 70"
			(at 8 -9.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Relay*SPDT*SANYOU*SRD*Series*Form*C*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "1"
			(at 0 -2.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "LINE")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.95 6.05 90)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 14.15 6.05 90)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LineRadiateur")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 14.2 -6 90)
			(size 3 3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(K1-Pad4)")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at 1.95 -5.95 90)
			(size 2.5 2.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 78.96 63.5)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "U2"
			(at 4.04 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "DS18B20"
			(at 1.04 3.8 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO*92*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J5-GCLK0{slash}GPIO4)")
			(pinfunction "DQ")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U2-VDD)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 36.92 48.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 5.08 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.58 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J5-GPIO23)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D2-GA)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 53.96 63.5 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "FAN"
			(at -2.7 1.34 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J9-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 88.58 33 90)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "J5"
			(at 1.27 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "ZeroHeader"
			(at 1.27 -50.59 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*")
		(sheetname "/")
		(sheetfile "Radiateur V2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -24.13 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(U2-VDD)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(J5-5V-Pad2)")
			(pinfunction "5V")
			(pintype "power_in+no_connect")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(J5-SDA{slash}GPIO2-Pad3)")
			(pinfunction "SDA/GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VCC")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J5-SCL{slash}GPIO3-Pad5)")
			(pinfunction "SCL/GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J5-GCLK0{slash}GPIO4)")
			(pinfunction "GCLK0/GPIO4")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J5-GPIO14{slash}TXD-Pad8)")
			(pinfunction "GPIO14/TXD")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" thru_hole oval
			(at 2.54 -10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J5-GPIO15{slash}RXD-Pad10)")
			(pinfunction "GPIO15/RXD")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J5-GPIO17)")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at 2.54 -12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(J5-GPIO18{slash}PWM0-Pad12)")
			(pinfunction "GPIO18/PWM0")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J5-GPIO27-Pad13)")
			(pinfunction "GPIO27")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole oval
			(at 2.54 -15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" thru_hole oval
			(at 0 -17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J5-GPIO22)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at 2.54 -17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J5-GPIO23)")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at 0 -20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J5-3V3-Pad17)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
		)
		(pad "18" thru_hole oval
			(at 2.54 -20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J5-GPIO24)")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 0 -22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J5-MOSI0{slash}GPIO10)")
			(pinfunction "MOSI0/GPIO10")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 2.54 -22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "21" thru_hole oval
			(at 0 -25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J5-MISO0{slash}GPIO9)")
			(pinfunction "MISO0/GPIO9")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 2.54 -25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(J5-GPIO25-Pad22)")
			(pinfunction "GPIO25")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole oval
			(at 0 -27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J5-SCLK0{slash}GPIO11-Pad23)")
			(pinfunction "SCLK0/GPIO11")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole oval
			(at 2.54 -27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J5-~{CE0}{slash}GPIO8-Pad24)")
			(pinfunction "~{CE0}/GPIO8")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole oval
			(at 0 -30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "26" thru_hole oval
			(at 2.54 -30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(J5-~{CE1}{slash}GPIO7-Pad26)")
			(pinfunction "~{CE1}/GPIO7")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole oval
			(at 0 -33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J5-ID_SD{slash}GPIO0-Pad27)")
			(pinfunction "ID_SD/GPIO0")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole oval
			(at 2.54 -33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(J5-ID_SC{slash}GPIO1-Pad28)")
			(pinfunction "ID_SC/GPIO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" thru_hole oval
			(at 0 -35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(J5-GCLK1{slash}GPIO5-Pad29)")
			(pinfunction "GCLK1/GPIO5")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" thru_hole oval
			(at 2.54 -35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 -38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J5-GCLK2{slash}GPIO6-Pad31)")
			(pinfunction "GCLK2/GPIO6")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" thru_hole oval
			(at 2.54 -38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J5-PWM0{slash}GPIO12-Pad32)")
			(pinfunction "PWM0/GPIO12")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" thru_hole oval
			(at 0 -40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J5-PWM1{slash}GPIO13-Pad33)")
			(pinfunction "PWM1/GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" thru_hole oval
			(at 2.54 -40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" thru_hole oval
			(at 0 -43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J5-GPIO19{slash}MISO1-Pad35)")
			(pinfunction "GPIO19/MISO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" thru_hole oval
			(at 2.54 -43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J5-GPIO16)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole oval
			(at 0 -45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J5-GPIO26-Pad37)")
			(pinfunction "GPIO26")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" thru_hole oval
			(at 2.54 -45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J5-GPIO20{slash}MOSI1-Pad38)")
			(pinfunction "GPIO20/MOSI1")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" thru_hole oval
			(at 0 -48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole oval
			(at 2.54 -48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(J5-GPIO21{slash}SCLK1-Pad40)")
			(pinfunction "GPIO21/SCLK1")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 35.43 58.27)
		(end 34.93 58.27)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 30.5 24.5)
		(end 140.5 69.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 93.43 54.77) (xy 93.43 31.77)
		)
		(height 7.5)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "0,9055 in"
			(at 99.13 43.27 90)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 35.43 31.77) (xy 64.43 31.77)
		)
		(height 7.2)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "1,1417 in"
			(at 49.93 37.17 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 31.93 54.77) (xy 35.43 54.77)
		)
		(height 6)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "0,1378 in"
			(at 33.68 58.97 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 96.53 54.77) (xy 90.33 54.77)
		)
		(height -9.6)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "0,2441 in"
			(at 93.43 62.57 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 93.43 31.77) (xy 35.43 31.77)
		)
		(height 7.5)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "2,2835 in"
			(at 64.43 22.47 0)
			(layer "Cmts.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 93.43 58.27) (xy 93.43 28.27)
		)
		(height 13)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "1,1811 in"
			(at 104.63 43.27 90)
			(layer "Cmts.User")
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 30.5 24.5) (xy 103.5 24.5) (xy 103.5 59) (xy 107 59) (xy 107 69) (xy 30.5 69.5)
			)
		)
	)
	(embedded_fonts no)
)
