(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 39)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.5)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 13.97 67.31)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00100_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(PS1-Pad1)")
  (net 4 "Net-(PS1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
  )
  (net_class AC ""
    (clearance 1.5)
    (trace_width 2)
    (via_dia 2.6)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(PS1-Pad1)")
    (add_net "Net-(PS1-Pad2)")
  )
  (module radiateur:PowerAdapt (layer B.Cu) (tedit 61B20D03)
    (at 129.54 95.25 180)
    (descr "Trafo, Printtrafo, CHK, EI30, 2VA, 1x Sec,http://www.eratransformers.com/downloads/030-7585.0.pdf")
    (tags "Trafo Printtrafo CHK EI30 2VA 1x Sec ")
    (fp_text reference T1 (at 10 27.78) (layer B.SilkS))
    (fp_text value Tranfo_Tagada-Device (at 10 10 270) (layer B.Fab))
    (fp_text user Sec (at 17 10 270) (layer B.SilkS))
    (fp_text user Pri (at 3 10 270) (layer B.SilkS))
    (fp_text user 9 (at 16 4 270) (layer B.Fab))
    (fp_text user 7 (at 16 16 270) (layer B.Fab))
    (fp_text user 5 (at 3 22 270) (layer B.Fab))
    (fp_text user 1 (at 3 -2 270) (layer B.SilkS))
    (fp_text user %R (at 10 24.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 20 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 20 10 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_CHK_EI30-2VA_1xSec.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:AZ_AC-05-3 (layer F.Cu) (tedit 61B204BA)
    (at 123.19 100.33 180)
    (descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT, https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF")
    (tags "ACDC-Converter 3W THT")
    (fp_text reference PS1 (at 8.89 -4.5) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 8.89 16.24) (layer F.Fab))
    (fp_text user %R (at 8.89 14.24) (layer F.Fab))
    (pad 4 thru_hole circle (at 17.78 25.4 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 17.78 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 5.08 180) (size 2.3 2.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.3 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-03-xx_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:dcconn (layer F.Cu) (tedit 61B21ADD)
    (at 99.06 100.33 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J1 (at 1.25 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -1.27 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:PowerAdapt (layer B.Cu) (tedit 61B20D03)
    (at 91.44 95.25 180)
    (descr "Trafo, Printtrafo, CHK, EI30, 2VA, 1x Sec,http://www.eratransformers.com/downloads/030-7585.0.pdf")
    (tags "Trafo Printtrafo CHK EI30 2VA 1x Sec ")
    (fp_text reference T1 (at 10 27.78) (layer B.SilkS))
    (fp_text value Tranfo_Tagada-Device (at 10 10 270) (layer B.Fab))
    (fp_text user Sec (at 17 10 270) (layer B.SilkS))
    (fp_text user Pri (at 3 10 270) (layer B.SilkS))
    (fp_text user 9 (at 16 4 270) (layer B.Fab))
    (fp_text user 7 (at 16 16 270) (layer B.Fab))
    (fp_text user 5 (at 3 22 270) (layer B.Fab))
    (fp_text user 1 (at 3 -2 270) (layer B.SilkS))
    (fp_text user %R (at 10 24.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 20 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 20 10 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_CHK_EI30-2VA_1xSec.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:AZ_AC-05-3 (layer F.Cu) (tedit 61B204BA)
    (at 85.09 100.33 180)
    (descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT, https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF")
    (tags "ACDC-Converter 3W THT")
    (fp_text reference PS1 (at 8.89 -4.5) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 8.89 16.24) (layer F.Fab))
    (fp_text user %R (at 8.89 14.24) (layer F.Fab))
    (pad 4 thru_hole circle (at 17.78 25.4 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 17.78 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 5.08 180) (size 2.3 2.3) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.3 2) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-03-xx_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:dcconn (layer F.Cu) (tedit 61B21ADD)
    (at 60.96 100.33 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J1 (at 1.25 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -1.27 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:dcconn (layer F.Cu) (tedit 61B21ADD)
    (at 22.86 100.33 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J1 (at 1.25 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole roundrect (at -1.27 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:PowerAdapt (layer B.Cu) (tedit 61B20D03)
    (at 53.34 95.25 180)
    (descr "Trafo, Printtrafo, CHK, EI30, 2VA, 1x Sec,http://www.eratransformers.com/downloads/030-7585.0.pdf")
    (tags "Trafo Printtrafo CHK EI30 2VA 1x Sec ")
    (fp_text reference T1 (at 10 27.78) (layer B.SilkS))
    (fp_text value Tranfo_Tagada-Device (at 10 10 270) (layer B.Fab))
    (fp_text user %R (at 10 24.5) (layer B.Fab))
    (fp_text user 1 (at 3 -2 270) (layer B.SilkS))
    (fp_text user 5 (at 3 22 270) (layer B.Fab))
    (fp_text user 7 (at 16 16 270) (layer B.Fab))
    (fp_text user 9 (at 16 4 270) (layer B.Fab))
    (fp_text user Pri (at 3 10 270) (layer B.SilkS))
    (fp_text user Sec (at 17 10 270) (layer B.SilkS))
    (pad 8 thru_hole circle (at 20 10 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 20 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(PS1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "Net-(PS1-Pad1)"))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_CHK_EI30-2VA_1xSec.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radiateur:AZ_AC-05-3 (layer F.Cu) (tedit 61B204BA)
    (at 46.99 100.33 180)
    (descr "ACDC-Converter, 3W, Meanwell, IRM-03, THT, https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF")
    (tags "ACDC-Converter 3W THT")
    (fp_text reference PS1 (at 8.89 -4.5) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 8.89 16.24) (layer F.Fab))
    (fp_text user %R (at 8.89 14.24) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.3 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(PS1-Pad1)"))
    (pad 2 thru_hole circle (at 0 5.08 180) (size 2.3 2.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(PS1-Pad2)"))
    (pad 3 thru_hole circle (at 17.78 30.48 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 17.78 25.4 180) (size 2.3 2.3) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Converter_ACDC.3dshapes/Converter_ACDC_MeanWell_IRM-03-xx_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (target plus (at 13.97 104.14) (size 5) (width 0.1) (layer Edge.Cuts))
  (target plus (at 15.24 67.31) (size 5) (width 0.1) (layer Edge.Cuts))
  (target plus (at 12.7 67.31) (size 5) (width 0.1) (layer Edge.Cuts))
)
