(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 137)
    (zones 0)
    (modules 20)
    (nets 47)
  )
  (page A4)
  (title_block
    (title "Radiateur PCB")
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.7)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 VCC)
  (net 4 "Net-(D1-Pad3)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad3)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 LINE)
  (net 11 NEUT)
  (net 12 "Net-(J5-Pad1)")
  (net 13 "Net-(Q1-Pad2)")
  (net 14 "Net-(J5-Pad11)")
  (net 15 "Net-(J5-Pad15)")
  (net 16 "Net-(J5-Pad16)")
  (net 17 "Net-(J5-Pad18)")
  (net 18 "Net-(J5-Pad7)")
  (net 19 "Net-(J5-Pad2)")
  (net 20 "Net-(J5-Pad3)")
  (net 21 "Net-(J5-Pad5)")
  (net 22 "Net-(J5-Pad8)")
  (net 23 "Net-(J5-Pad10)")
  (net 24 "Net-(J5-Pad12)")
  (net 25 "Net-(J5-Pad13)")
  (net 26 "Net-(J5-Pad17)")
  (net 27 "Net-(J5-Pad19)")
  (net 28 "Net-(J5-Pad21)")
  (net 29 "Net-(J5-Pad22)")
  (net 30 "Net-(J5-Pad23)")
  (net 31 "Net-(J5-Pad24)")
  (net 32 "Net-(J5-Pad26)")
  (net 33 "Net-(J5-Pad27)")
  (net 34 "Net-(J5-Pad28)")
  (net 35 "Net-(J5-Pad29)")
  (net 36 "Net-(J5-Pad31)")
  (net 37 "Net-(J5-Pad32)")
  (net 38 "Net-(J5-Pad33)")
  (net 39 "Net-(J5-Pad35)")
  (net 40 "Net-(J5-Pad36)")
  (net 41 "Net-(J5-Pad37)")
  (net 42 "Net-(J5-Pad38)")
  (net 43 "Net-(J5-Pad40)")
  (net 44 /LineRadiateur)
  (net 45 "Net-(K1-Pad4)")
  (net 46 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.7)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad11)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad15)")
    (add_net "Net-(J5-Pad16)")
    (add_net "Net-(J5-Pad17)")
    (add_net "Net-(J5-Pad18)")
    (add_net "Net-(J5-Pad19)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad21)")
    (add_net "Net-(J5-Pad22)")
    (add_net "Net-(J5-Pad23)")
    (add_net "Net-(J5-Pad24)")
    (add_net "Net-(J5-Pad26)")
    (add_net "Net-(J5-Pad27)")
    (add_net "Net-(J5-Pad28)")
    (add_net "Net-(J5-Pad29)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad31)")
    (add_net "Net-(J5-Pad32)")
    (add_net "Net-(J5-Pad33)")
    (add_net "Net-(J5-Pad35)")
    (add_net "Net-(J5-Pad36)")
    (add_net "Net-(J5-Pad37)")
    (add_net "Net-(J5-Pad38)")
    (add_net "Net-(J5-Pad40)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net VCC)
  )
  (net_class 220V ""
    (clearance 1.5)
    (trace_width 2.5)
    (via_dia 2)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LineRadiateur)
    (add_net LINE)
    (add_net NEUT)
  )
  (module LED_THT:LED_RGB_5mm_amazon (layer F.Cu) (tedit 5DB20115)
    (at 64.77 35.56)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED")
    (fp_text reference D2 (at 3.2385 -3.96) (layer F.SilkS))
    (fp_text value LED_RGBC (at 3.2385 3.96) (layer F.Fab))
    (fp_text user %R (at 3.2385 -3.96) (layer F.Fab))
    (pad 4 thru_hole circle (at 2.032 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 7.112 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad3)"))
    (pad 2 thru_hole circle (at 4.572 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at -0.508 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm-4_RGB_Wide_Pins.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 83.82 46.99 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 3.81 -2.12 90) (layer F.SilkS))
    (fp_text value 1N4448 (at 3.81 2.12 90) (layer F.Fab))
    (fp_text user %R (at 4.11 0 90) (layer F.Fab))
    (fp_text user K (at 0 -1.8 90) (layer F.Fab))
    (fp_text user K (at 0 -1.8 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92L_Inline_Wide (layer F.Cu) (tedit 5A11996A)
    (at 81.28 35.56 180)
    (descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
    (tags "TO-92L Inline Wide transistor")
    (fp_text reference U2 (at 2.54 -3.56) (layer F.SilkS))
    (fp_text value DS18B20 (at 2.54 2.79) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad7)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92L_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A02FF81)
    (at 72.39 54.61 270)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.56 90) (layer F.SilkS))
    (fp_text value 2N2222 (at 2.54 2.79 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.56 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 52.07 54.61)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 4K7 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad11)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork (layer F.Cu) (tedit 5A1DC085)
    (at 115.57 43.18)
    (descr "solder Pin_ with flat with fork, hole diameter 1.2mm, length 11.3mm, width 3.0mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J4 (at 0 2.2) (layer F.SilkS))
    (fp_text value RadiateurIn (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 /LineRadiateur))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork (layer F.Cu) (tedit 5A1DC085)
    (at 115.57 77.47)
    (descr "solder Pin_ with flat with fork, hole diameter 1.2mm, length 11.3mm, width 3.0mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J3 (at 0 2.2) (layer F.SilkS))
    (fp_text value RadiateurOut (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 NEUT))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork (layer F.Cu) (tedit 5A1DC085)
    (at 115.57 66.04)
    (descr "solder Pin_ with flat with fork, hole diameter 1.2mm, length 11.3mm, width 3.0mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J2 (at 0 2.2) (layer F.SilkS))
    (fp_text value Neutral (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 NEUT))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Pin:Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork (layer F.Cu) (tedit 5A1DC085)
    (at 115.57 54.61)
    (descr "solder Pin_ with flat with fork, hole diameter 1.2mm, length 11.3mm, width 3.0mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference J1 (at 0 2.2) (layer F.SilkS))
    (fp_text value Line (at 0 -2.05) (layer F.Fab))
    (fp_text user %R (at 0 2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 LINE))
    (model ${KISYS3DMOD}/Connector_Pin.3dshapes/Pin_D1.2mm_L10.2mm_W2.9mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148)
    (at 90.61 39.37)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K1 (at 8.1 9.2) (layer F.SilkS))
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 LINE))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 45 "Net-(K1-Pad4)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 /LineRadiateur))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D8.0mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 39.305001 56.295001)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 8mm width 5.0mm Capacitor")
    (fp_text reference C1 (at 2.5 -3.75) (layer F.SilkS))
    (fp_text value 330nF (at 2.5 3.75) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D8.0mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D8.0mm_W5.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 29.755001 56.295001)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=8*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 8mm width 5.0mm Capacitor")
    (fp_text reference C2 (at 2.5 -3.75) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 3.75) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D8.0mm_W5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:Diode_Bridge_Vishay_KBU (layer F.Cu) (tedit 5A4F7739)
    (at 53.34 73.66)
    (descr "Vishay KBU rectifier package, 5.08mm pitch, see http://www.vishay.com/docs/88656/kbu4.pdf")
    (tags "Vishay KBU rectifier diode bridge")
    (fp_text reference D1 (at 7.8 -3.1) (layer F.SilkS))
    (fp_text value KBU4M (at 7.5 6.2) (layer F.Fab))
    (fp_text user %R (at 7.7 3.3) (layer F.Fab))
    (pad 4 thru_hole circle (at 15.24 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 10.16 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/Diode_Bridge_Vishay_KBU.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 62.23 64.77 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 470 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 52.07 60.0075)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad15)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 49.53 36.83)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad16)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 45.72 36.83 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad18)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 39.37 74.93 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U1 (at 2.54 -4.27) (layer F.SilkS))
    (fp_text value L7805 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 76.2 44.45 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J5 (at 1.27 2.33 270) (layer B.SilkS))
    (fp_text value ZeroHeader (at 1.27 -50.59 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -24.13) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J5-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J5-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 -22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J5-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 -25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 -27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad24)"))
    (pad 25 thru_hole oval (at 0 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 -30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 -33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad28)"))
    (pad 29 thru_hole oval (at 0 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 -35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 -38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad32)"))
    (pad 33 thru_hole oval (at 0 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 -40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 -43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad36)"))
    (pad 37 thru_hole oval (at 0 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 -45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J5-Pad38)"))
    (pad 39 thru_hole oval (at 0 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 -48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J5-Pad40)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformer_THT:Transformer_CHK_EI30-2VA_1xSec (layer F.Cu) (tedit 5BEAEA14)
    (at 109.22 55.88 180)
    (descr "Trafo, Printtrafo, CHK, EI30, 2VA, 1x Sec,http://www.eratransformers.com/downloads/030-7585.0.pdf")
    (tags "Trafo Printtrafo CHK EI30 2VA 1x Sec ")
    (fp_text reference T1 (at 10 -27.78) (layer F.SilkS))
    (fp_text value Tranfo_Tagada (at 10 -10 90) (layer F.Fab))
    (fp_text user Sec (at 17 -10 90) (layer F.SilkS))
    (fp_text user Pri (at 3 -10 90) (layer F.SilkS))
    (fp_text user 9 (at 16 -4 90) (layer F.Fab))
    (fp_text user 7 (at 16 -16 90) (layer F.Fab))
    (fp_text user 5 (at 3 -22 90) (layer F.Fab))
    (fp_text user 1 (at 3 2 90) (layer F.SilkS))
    (fp_text user %R (at 10 -24.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 10 LINE))
    (pad 2 thru_hole circle (at 0 -5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 -10 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 0 -15 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 -20 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 11 NEUT))
    (pad 6 thru_hole circle (at 20 -20 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 20 -15 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad3)"))
    (pad 8 thru_hole circle (at 20 -10 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 20 -5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 10 thru_hole circle (at 20 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Transformer_THT.3dshapes/Transformer_CHK_EI30-2VA_1xSec.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 119.38 29.21) (end 20.32 29.21) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.38 83.82) (end 119.38 29.21) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 20.32 83.82) (end 119.38 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 20.32 29.21) (end 20.32 83.82) (layer Edge.Cuts) (width 0.1))
  (gr_text "Radiateur Board V1" (at 38.1 81.28) (layer F.Cu))
  (dimension 99.06 (width 0.12) (layer F.SilkS)
    (gr_text "99.060 mm" (at 69.85 21.59) (layer F.SilkS))
    (feature1 (pts (xy 119.38 29.21) (xy 119.38 22.273579)))
    (feature2 (pts (xy 20.32 29.21) (xy 20.32 22.273579)))
    (crossbar (pts (xy 20.32 22.86) (xy 119.38 22.86)))
    (arrow1a (pts (xy 119.38 22.86) (xy 118.253496 23.446421)))
    (arrow1b (pts (xy 119.38 22.86) (xy 118.253496 22.273579)))
    (arrow2a (pts (xy 20.32 22.86) (xy 21.446504 23.446421)))
    (arrow2b (pts (xy 20.32 22.86) (xy 21.446504 22.273579)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 20.32 29.21) (xy 119.38 29.21) (xy 119.38 83.82) (xy 20.32 83.82)
      )
    )
  )
)
