(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:GND-power"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "power_GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "GND-power_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND-power_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:C"
			(pin_names
				(offset 0.254)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 0.635 2.54 0)
			)
			(property "Value" "C"
				(at 0.635 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Condensateur non polarise"
				(at 0 0 0)
			)
			(symbol "C_0_1"
				(polyline
					(pts
						(xy -2.032 0.762)
						(xy 2.032 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762)
						(xy 2.032 -0.762)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "C_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "power:+3V3"
			(power)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3V3"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Alimentation +3V3"
				(at 0 0 0)
			)
			(symbol "+3V3_0_1"
				(polyline
					(pts
						(xy -0.762 1.27)
						(xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0)
						(xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54)
						(xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3V3_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "+3V3")
					(number "1")
				)
			)
		)
		(symbol "ir-test:TSOP4838"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 11.43 0)
			)
			(property "Value" "TSOP4838"
				(at -5.08 13.97 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Recepteur IR 38 kHz Vishay TSOP4838 (symbole cree pour ce test)"
				(at 0 0 0)
			)
			(symbol "TSOP4838_0_1"
				(rectangle
					(start -5.08 5.08)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -5.08 2.54)
						(xy -7.62 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0)
						(xy -7.62 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 -2.54)
						(xy -7.62 -2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "TSOP4838_1_1"
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "OUT")
					(number "1")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VS")
					(number "3")
				)
			)
		)
		(symbol "ir-test:ESP32-DevKitV1"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -12.7 22.86 0)
			)
			(property "Value" "ESP32-DevKitV1"
				(at -12.7 25.4 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Module ESP32 DevKit V1 30 broches (symbole cree pour ce test)"
				(at 0 0 0)
			)
			(symbol "ESP32-DevKitV1_0_1"
				(rectangle
					(start -12.7 20.32)
					(end 12.7 -20.32)
					(fill
						(type background)
					)
				)
			)
			(symbol "ESP32-DevKitV1_1_1"
				(pin bidirectional line
					(at -15.24 17.78 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin bidirectional line
					(at -15.24 15.24 0)
					(length 2.54)
					(name "GPIO36")
					(number "2")
				)
				(pin bidirectional line
					(at -15.24 12.7 0)
					(length 2.54)
					(name "GPIO39")
					(number "3")
				)
				(pin bidirectional line
					(at -15.24 10.16 0)
					(length 2.54)
					(name "GPIO34")
					(number "4")
				)
				(pin bidirectional line
					(at -15.24 7.62 0)
					(length 2.54)
					(name "GPIO35")
					(number "5")
				)
				(pin bidirectional line
					(at -15.24 5.08 0)
					(length 2.54)
					(name "GPIO32")
					(number "6")
				)
				(pin bidirectional line
					(at -15.24 2.54 0)
					(length 2.54)
					(name "GPIO33")
					(number "7")
				)
				(pin bidirectional line
					(at -15.24 0 0)
					(length 2.54)
					(name "GPIO25")
					(number "8")
				)
				(pin bidirectional line
					(at -15.24 -2.54 0)
					(length 2.54)
					(name "GPIO26")
					(number "9")
				)
				(pin bidirectional line
					(at -15.24 -5.08 0)
					(length 2.54)
					(name "GPIO27")
					(number "10")
				)
				(pin bidirectional line
					(at -15.24 -7.62 0)
					(length 2.54)
					(name "GPIO14")
					(number "11")
				)
				(pin bidirectional line
					(at -15.24 -10.16 0)
					(length 2.54)
					(name "GPIO12")
					(number "12")
				)
				(pin power_in line
					(at -15.24 -12.7 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at -15.24 -15.24 0)
					(length 2.54)
					(name "GPIO13")
					(number "14")
				)
				(pin power_in line
					(at -15.24 -17.78 0)
					(length 2.54)
					(name "VIN")
					(number "15")
				)
				(pin power_in line
					(at 15.24 17.78 180)
					(length 2.54)
					(name "3V3")
					(number "16")
				)
				(pin power_in line
					(at 15.24 15.24 180)
					(length 2.54)
					(name "GND")
					(number "17")
				)
				(pin bidirectional line
					(at 15.24 12.7 180)
					(length 2.54)
					(name "GPIO15")
					(number "18")
				)
				(pin bidirectional line
					(at 15.24 10.16 180)
					(length 2.54)
					(name "GPIO2")
					(number "19")
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 2.54)
					(name "GPIO4")
					(number "20")
				)
				(pin bidirectional line
					(at 15.24 5.08 180)
					(length 2.54)
					(name "GPIO16")
					(number "21")
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 2.54)
					(name "GPIO17")
					(number "22")
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 2.54)
					(name "GPIO5")
					(number "23")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "GPIO18")
					(number "24")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "GPIO19")
					(number "25")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 2.54)
					(name "GPIO21")
					(number "26")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 2.54)
					(name "GPIO3")
					(number "27")
				)
				(pin bidirectional line
					(at 15.24 -12.7 180)
					(length 2.54)
					(name "GPIO1")
					(number "28")
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 2.54)
					(name "GPIO22")
					(number "29")
				)
				(pin bidirectional line
					(at 15.24 -17.78 180)
					(length 2.54)
					(name "GPIO23")
					(number "30")
				)
			)
		)
	)
	(junction
		(at 114.3 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 114.3 63.5) (xy 114.3 67.31)
		)
	)
	(wire
		(pts
			(xy 114.3 74.93) (xy 114.3 81.28)
		)
	)
	(wire
		(pts
			(xy 99.06 81.28) (xy 114.3 81.28)
		)
	)
	(wire
		(pts
			(xy 99.06 88.9) (xy 99.06 92.71)
		)
	)
	(wire
		(pts
			(xy 114.3 96.52) (xy 114.3 100.33)
		)
	)
	(wire
		(pts
			(xy 121.92 88.9) (xy 129.54 88.9)
		)
	)
	(wire
		(pts
			(xy 180.34 83.82) (xy 187.96 83.82)
		)
	)
	(wire
		(pts
			(xy 180.34 71.12) (xy 185.42 71.12)
		)
	)
	(wire
		(pts
			(xy 185.42 71.12) (xy 185.42 67.31)
		)
	)
	(wire
		(pts
			(xy 149.86 101.6) (xy 185.42 73.66)
		)
	)
	(wire
		(pts
			(xy 185.42 73.66) (xy 185.42 77.47)
		)
	)
	(label "IR_RX"
		(at 129.54 88.9 0)
	)
	(label "IR_RX"
		(at 187.96 83.82 0)
	)
	(symbol
		(lib_id "ir-test:ESP32-DevKitV1")
		(at 165.1 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U1"
			(at 168.91 87.63 0)
		)
		(property "Value" "ESP32-DevKitV1"
			(at 168.91 90.17 0)
		)
		(property "Footprint" ""
			(at 165.1 88.9 0)
		)
		(property "Datasheet" ""
			(at 165.1 88.9 0)
		)
		(property "Description" ""
			(at 165.1 88.9 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "26")
		(pin "27")
		(pin "28")
		(pin "29")
		(pin "30")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "ir-test:TSOP4838")
		(at 114.3 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 118.11 87.63 0)
		)
		(property "Value" "TSOP4838"
			(at 118.11 90.17 0)
		)
		(property "Footprint" ""
			(at 114.3 88.9 0)
		)
		(property "Datasheet" ""
			(at 114.3 88.9 0)
		)
		(property "Description" ""
			(at 114.3 88.9 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 114.3 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 118.11 69.85 0)
		)
		(property "Value" "100R"
			(at 118.11 72.39 0)
		)
		(property "Footprint" ""
			(at 114.3 71.12 0)
		)
		(property "Datasheet" ""
			(at 114.3 71.12 0)
		)
		(property "Description" ""
			(at 114.3 71.12 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:C")
		(at 99.06 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C1"
			(at 102.87 83.82 0)
		)
		(property "Value" "4.7uF"
			(at 102.87 86.36 0)
		)
		(property "Footprint" ""
			(at 99.06 85.09 0)
		)
		(property "Datasheet" ""
			(at 99.06 85.09 0)
		)
		(property "Description" ""
			(at 99.06 85.09 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3V3")
		(at 114.3 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01"
			(at 114.3 57.15 0)
		)
		(property "Value" "+3V3"
			(at 114.3 67.056 0)
		)
		(property "Footprint" ""
			(at 114.3 63.5 0)
		)
		(property "Datasheet" ""
			(at 114.3 63.5 0)
		)
		(property "Description" ""
			(at 114.3 63.5 0)
		)
		(pin "1")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+3V3")
		(at 185.42 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 185.42 60.96 0)
		)
		(property "Value" "+3V3"
			(at 185.42 70.866 0)
		)
		(property "Footprint" ""
			(at 185.42 67.31 0)
		)
		(property "Datasheet" ""
			(at 185.42 67.31 0)
		)
		(property "Description" ""
			(at 185.42 67.31 0)
		)
		(pin "1")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 99.06 92.71 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 99.06 86.36 0)
		)
		(property "Value" "power_GND"
			(at 99.06 88.9 0)
		)
		(property "Footprint" ""
			(at 99.06 92.71 0)
		)
		(property "Datasheet" ""
			(at 99.06 92.71 0)
		)
		(property "Description" ""
			(at 99.06 92.71 0)
		)
		(pin "1")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 114.3 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR04"
			(at 114.3 93.98 0)
		)
		(property "Value" "power_GND"
			(at 114.3 96.52 0)
		)
		(property "Footprint" ""
			(at 114.3 100.33 0)
		)
		(property "Datasheet" ""
			(at 114.3 100.33 0)
		)
		(property "Description" ""
			(at 114.3 100.33 0)
		)
		(pin "1")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 185.42 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 185.42 71.12 0)
		)
		(property "Value" "power_GND"
			(at 185.42 73.66 0)
		)
		(property "Footprint" ""
			(at 185.42 77.47 0)
		)
		(property "Datasheet" ""
			(at 185.42 77.47 0)
		)
		(property "Description" ""
			(at 185.42 77.47 0)
		)
		(pin "1")
		(instances
			(project "ir-esp32-test"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
