(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
	)
	(net 0 "")
	(gr_text "REGLETTE ENTRAXE DFPLAYER MINI"
		(at 30 16 0)
		(layer "F.Cu")
	)
	(gr_text "poser le module a la loupe - lire l'entraxe centre sur LES DEUX rangees"
		(at 30 19.5 0)
		(layer "F.Cu")
	)
	(gr_text "17.80"
		(at 30 30 0)
		(layer "F.Cu")
	)
	(gr_text "17.90"
		(at 60 30 0)
		(layer "F.Cu")
	)
	(gr_text "18.00"
		(at 90 30 0)
		(layer "F.Cu")
	)
	(gr_text "18.10"
		(at 30 62 0)
		(layer "F.Cu")
	)
	(gr_text "18.20"
		(at 60 62 0)
		(layer "F.Cu")
	)
	(gr_text "18.30"
		(at 90 62 0)
		(layer "F.Cu")
	)
	(gr_text "echelle X : 20 pas de 2.54 = 50.80 mm (mesurer d'axe en axe)"
		(at 55.4 91 0)
		(layer "F.Cu")
	)
	(gr_text "echelle Y : 50.80 mm"
		(at 94.8 91 0)
		(layer "F.Cu")
	)
	(gr_line
		(start 14.95 12)
		(end 105.15 12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.15 12)
		(end 105.15 150.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.15 150.8)
		(end 14.95 150.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 14.95 150.8)
		(end 14.95 12)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
