(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 50 93)
		(grid_origin 50 50)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "GND")
	(net 3 "+3V3")
	(net 4 "/SPK2")
	(net 5 "/GPIO0")
	(net 6 "/RXD0")
	(net 7 "/TXD0")
	(net 8 "/RST")
	(net 9 "Net-(U1-EN)")
	(net 10 "Net-(U1-GPIO15)")
	(net 11 "/DF_RX")
	(net 12 "Net-(U3-RX)")
	(net 13 "Net-(U1-GPIO2)")
	(net 14 "unconnected-(U1-MOSI-Pad13)")
	(net 15 "unconnected-(U1-GPIO16-Pad4)")
	(net 16 "unconnected-(U1-MISO-Pad10)")
	(net 17 "unconnected-(U1-GPIO12-Pad6)")
	(net 18 "unconnected-(U1-GPIO10-Pad12)")
	(net 19 "unconnected-(U1-GPIO13-Pad7)")
	(net 20 "unconnected-(U1-SCLK-Pad14)")
	(net 21 "unconnected-(U1-GPIO9-Pad11)")
	(net 22 "/DF_BUSY")
	(net 23 "unconnected-(U1-CS0-Pad9)")
	(net 24 "unconnected-(U1-ADC-Pad2)")
	(net 25 "unconnected-(U3-ADKEY_1-Pad12)")
	(net 26 "unconnected-(U3-DAC_L-Pad5)")
	(net 27 "unconnected-(U3-IO_2-Pad11)")
	(net 28 "unconnected-(U3-USB--Pad15)")
	(net 29 "unconnected-(U3-IO_1-Pad9)")
	(net 30 "unconnected-(U3-ADKEY_2-Pad13)")
	(net 31 "unconnected-(U3-DAC_R-Pad4)")
	(net 32 "unconnected-(U3-USB+-Pad14)")
	(net 33 "/SPK1")
	(net 34 "/DF_TX")
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 65.5 75 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 1.25 -4.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 1.25 4.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 54 55)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Entree 5 V"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm"
		(layer "F.Cu")
		(at 65 86 90)
		(descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 1.75 -5.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "220uF"
			(at 1.75 5.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 56 87.5 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 2.5 -2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.5 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 94.84 52.5 90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Prog + auto-reset"
			(at 0 12.49 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TXD0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/RXD0")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GPIO0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/RST")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 80 90.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(U1-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 95 90.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-GPIO2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 85 90.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GPIO0")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "sonnette:ESP-12F_Castellated"
		(layer "F.Cu")
		(at 77.5 55.8)
		(descr "ESP-12F soude en CMS sur ses bords castelles. Pads de X=6.6 a 9.6 : 1.4 mm sous le module, 1.6 mm accessibles au fer. Trou de via 0.7 mm a X=+/-8.95, HORS du module pour ne pas drainer le joint. 6 pads de flash non connectes. Zone antenne 6.2 mm : AUCUN cuivre, aucune couche.")
		(tags "ESP-12F ESP8266 THT castellated Ai-Thinker")
		(property "Reference" "U1"
			(at 0 -13.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESP-12F"
			(at 0 13.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ESP?12*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -9.75 -3.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/RST")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at -9.75 -1.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-ADC-Pad2)")
			(pinfunction "ADC")
			(pintype "input+no_connect")
		)
		(pad "3" thru_hole oval
			(at -9.75 0.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(U1-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at -9.75 2.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-GPIO16-Pad4)")
			(pinfunction "GPIO16")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole oval
			(at -9.75 4.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/DF_BUSY")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at -9.75 6.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-GPIO12-Pad6)")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole oval
			(at -9.75 8.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-GPIO13-Pad7)")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole oval
			(at -9.75 10.5)
			(size 3 1.3)
			(drill 0.8
				(offset 0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at -5 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(U1-CS0-Pad9)")
			(pinfunction "CS0")
			(pintype "input+no_connect")
		)
		(pad "10" smd rect
			(at -3 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(U1-MISO-Pad10)")
			(pinfunction "MISO")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd rect
			(at -1 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1-GPIO9-Pad11)")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd rect
			(at 1 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(U1-GPIO10-Pad12)")
			(pinfunction "GPIO10")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd rect
			(at 3 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(U1-MOSI-Pad13)")
			(pinfunction "MOSI")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" smd rect
			(at 5 12)
			(size 1 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-SCLK-Pad14)")
			(pinfunction "SCLK")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole oval
			(at 9.75 10.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" thru_hole oval
			(at 9.75 8.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(U1-GPIO15)")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at 9.75 6.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1-GPIO2)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 9.75 4.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GPIO0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 9.75 2.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DF_RX")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 9.75 0.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/DF_TX")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 9.75 -1.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/RXD0")
			(pinfunction "GPIO3/RXD")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 9.75 -3.5)
			(size 3 1.3)
			(drill 0.8
				(offset -0.8 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/TXD0")
			(pinfunction "GPIO1/TXD")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 105 90.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U3-RX)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DF_RX")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 127.5 85 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "HP 8 ohms"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/SPK1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/SPK2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 90 90.08 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/RST")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 100 79.92 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(U1-GPIO15)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "sonnette:DFPlayer_Mini"
		(layer "F.Cu")
		(at 120 65 90)
		(descr "DFPlayer Mini, lecteur MP3 microSD. 2x8 broches, pas 2.54 mm, entraxe des rangees 17.78 mm, carte ~20 x 20 mm.")
		(tags "DFPlayer MP3 module THT 2x8 2.54mm")
		(property "Reference" "U3"
			(at 0 -11.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "DFPlayer Mini"
			(at 0 11.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -9.05 -8.89 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at -9.05 -6.35 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U3-RX)")
			(pinfunction "RX")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at -9.05 -3.81 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/DF_TX")
			(pinfunction "TX")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at -9.05 -1.27 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(U3-DAC_R-Pad4)")
			(pinfunction "DAC_R")
			(pintype "output+no_connect")
		)
		(pad "5" thru_hole oval
			(at -9.05 1.27 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U3-DAC_L-Pad5)")
			(pinfunction "DAC_L")
			(pintype "output+no_connect")
		)
		(pad "6" thru_hole oval
			(at -9.05 3.81 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/SPK1")
			(pinfunction "SPK_1")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at -9.05 6.35 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at -9.05 8.89 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/SPK2")
			(pinfunction "SPK_2")
			(pintype "output")
		)
		(pad "9" thru_hole oval
			(at 9.05 8.89 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(U3-IO_1-Pad9)")
			(pinfunction "IO_1")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" thru_hole oval
			(at 9.05 6.35 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 9.05 3.81 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(U3-IO_2-Pad11)")
			(pinfunction "IO_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole oval
			(at 9.05 1.27 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(U3-ADKEY_1-Pad12)")
			(pinfunction "ADKEY_1")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole oval
			(at 9.05 -1.27 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(U3-ADKEY_2-Pad13)")
			(pinfunction "ADKEY_2")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole oval
			(at 9.05 -3.81 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U3-USB+-Pad14)")
			(pinfunction "USB+")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" thru_hole oval
			(at 9.05 -6.35 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U3-USB--Pad15)")
			(pinfunction "USB-")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole oval
			(at 9.05 -8.89 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/DF_BUSY")
			(pinfunction "BUSY")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 56 69.92)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "U2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "AMS1117-3.3 (module)"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Note" "OUT = broche du MILIEU. Lire la serigraphie : VIN et GND varient selon les lots, une inversion detruit le regulateur."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "/")
		(sheetfile "sonnette.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 131 50)
		(end 131 93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50 93)
		(end 50 50)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 50 50)
		(end 131 50)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131 93)
		(end 50 93)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 50 50) (xy 50 93) (xy 131 93) (xy 131 50)
			)
		)
	)
	(embedded_fonts no)
)
