(footprint "BatteryHolder_Bulgin_BX0036_1xC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bulgin Battery Holder, BX0036, Battery Type C (https://www.bulgin.com/products/pub/media/bulgin/data/Battery_holders.pdf)")
	(tags "Bulgin BX0036")
	(property "Reference" "REF**"
		(at 27.8 -18.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Bulgin_BX0036_1xC"
		(at 27.8 1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at 3 -0.2 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 27.8 -1 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 11.9 0)
		(size 3.8 3.8)
		(drill 3.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 43.7 0)
		(size 3.8 3.8)
		(drill 3.8)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 55.6 0)
		(size 2.6 2.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Bulgin_BX0036_1xC.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
