(footprint "BatteryHolder_ComfortableElectronic_CH273-2450_1x2450"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Comfortable Electronic CR2450 battery holder, http://www.comf.com.tw/ProductDetail.asp?no=148")
	(tags "Comfortable Electronic CR2450")
	(property "Reference" "REF**"
		(at 0.1 -6.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_ComfortableElectronic_CH273-2450_1x2450"
		(at 13.47 2.54 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 14 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 270)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 20 0 270)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_ComfortableElectronic_CH273-2450_1x2450.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
