(footprint "BatteryHolder_Keystone_2468_2xAAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2xAAA cell battery holder, Keystone P/N 2468, http://www.keyelco.com/product-pdf.cfm?p=1033")
	(tags "AAA battery cell holder")
	(property "Reference" "REF**"
		(at 0 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Keystone_2468_2xAAA"
		(at 23.9 7.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at 12.7 12.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 35.1 12.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -3.81 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 12.7 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at -3.81 12.7 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 35.1 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 23.9 5.35 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 8.64 4)
		(size 3.45 3.45)
		(drill 3.45)
		(layers "*.Cu")
	)
	(pad "" np_thru_hole circle
		(at 38.61 8.7)
		(size 3.45 3.45)
		(drill 3.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 12.7)
		(size 2 2)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2468_2xAAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
