(footprint "BatteryHolder_LINX_BAT-HLD-012-SMT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMT battery holder for CR1216/1220/1225, https://linxtechnologies.com/wp/wp-content/uploads/bat-hld-012-smt.pdf")
	(tags "battery holder coin cell cr1216 cr1220 cr1225")
	(property "Reference" "REF**"
		(at 0 6 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_LINX_BAT-HLD-012-SMT"
		(at 0 -7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.6 0)
		(size 2.5 5.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 7.6 0)
		(size 2.5 5.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd circle
		(at 0 0)
		(size 10.2 10.2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_LINX_BAT-HLD-012-SMT.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
