(footprint "BatteryHolder_MPD_BA9VPC_1xPP3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1xPP3 (9V) battery holder, Memory Protection Devices P/N BA9VPC, http://www.memoryprotectiondevices.com/datasheets/BA9VPC-datasheet.pdf")
	(tags "PP3 Battery Holder BA9VPC 9V")
	(property "Reference" "REF**"
		(at 0 -7.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_MPD_BA9VPC_1xPP3"
		(at 25.75 23.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at 3.6 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 3.6 12.88 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 25.75 6.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 12.29 17.62)
		(size 2.3 2.3)
		(drill 2.29)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 25.78 -4.73)
		(size 2.3 2.3)
		(drill 2.29)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 39.26 17.62)
		(size 2.3 2.3)
		(drill 2.29)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.41 4.02)
		(drill oval 0.66 2.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 12.88)
		(size 2.41 4.02)
		(drill oval 0.66 2.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_MPD_BA9VPC_1xPP3.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
