(footprint "BatteryHolder_MPD_BC12AAPC_2xAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2xAA cell battery holder, Memory Protection Devices P/N BC12AAPC, http://www.memoryprotectiondevices.com/datasheets/BC12AAPC-datasheet.pdf")
	(tags "AA battery cell holder")
	(property "Reference" "REF**"
		(at 51 -9.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_MPD_BC12AAPC_2xAA"
		(at 51 9.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at 14.705 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -4.4 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 106.4 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 36.295 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 87.295 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 65.705 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 51 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 26.15 -4.75)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 26.15 4.75)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 75.85 -4.75)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 75.85 4.75)
		(size 2.5 2.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.23 2.23)
		(drill 1.23)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 102 0)
		(size 2.23 2.23)
		(drill 1.23)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_MPD_BC12AAPC_2xAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
