(footprint "BatteryHolder_MPD_BC2AAPC_2xAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2xAA cell battery holder, Memory Protection Devices P/N BC2AAPC, http://www.memoryprotectiondevices.com/datasheets/BC2AAPC-datasheet.pdf")
	(tags "AA battery cell holder")
	(property "Reference" "REF**"
		(at 26.16 -10.11 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_MPD_BC2AAPC_2xAA"
		(at 26.16 23.39 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at -4.34 13.59 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 36.955 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 15.365 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 15.365 13.59 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -4.34 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at 36.955 13.59 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 26.16 6.63 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 26.16 6.63)
		(size 3.65 3.65)
		(drill 3.65)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.17 2.17)
		(drill 1.17)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 13.59)
		(size 2.17 2.17)
		(drill 1.17)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_MPD_BC2AAPC_2xAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
