(footprint "BatteryHolder_MYOUNG_BS-07-A1BJ001_CR2032"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CR2032 battery holder https://www.lcsc.com/datasheet/lcsc_datasheet_2203021630_MYOUNG-BS-07-A1BJ001_C2979167.pdf")
	(tags "CR2032 BR2032 BatteryHolder Battery")
	(property "Reference" "REF**"
		(at -1.5 -4.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_MYOUNG_BS-07-A1BJ001_CR2032"
		(at 12.4 13 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 12.4 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 12.4 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.4 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 20.8 0 180)
		(size 2 2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_MYOUNG_BS-07-A1BJ001_CR2032.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
