(footprint "Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic CR-1220/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D140.PDF")
	(tags "battery CR-1220 coin cell vertical")
	(property "Reference" "REF**"
		(at 1.625 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles"
		(at 1.625 1.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -1.46 -0.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 1.625 -1.2 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 1.6 1.6)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3.25 -2.45)
		(size 1.6 1.6)
		(drill 1.09)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
