(footprint "Battery_Panasonic_CR3032-VCN_Vertical_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic CR-3032/VCN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D508.PDF")
	(tags "battery CR-3032 coin cell vertical")
	(property "Reference" "REF**"
		(at 4.325 -6.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Battery_Panasonic_CR3032-VCN_Vertical_CircularHoles"
		(at 4.325 2.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -2.7 -0.75 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 4.325 -1.95 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3.7 3.7)
		(drill 3.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 9.15 -3.9)
		(size 2.7 2.7)
		(drill 2.12)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/Battery_Panasonic_CR3032-VCN_Vertical_CircularHoles.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
