(footprint "SW_Cherry_MX_6.25u_Plate"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Cherry MX keyswitch, 6.25u, plate mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
	(tags "Cherry MX keyswitch 6.25u plate")
	(property "Reference" "REF**"
		(at -2.54 -2.794 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Cherry_MX_6.25u_Plate"
		(at -2.54 12.954 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2.54 -2.794 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.54 5.08)
		(size 4 4)
		(drill 4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -6.35 2.54)
		(size 2.2 2.2)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_6.25u_Plate.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
