(footprint "SW_DIP_SPSTx09_Slide_Omron_A6S-910x_W8.9mm_P2.54mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SMD 9x-dip-switch SPST Omron_A6S-910x, Slide, row spacing 8.9 mm (350 mils), body size  (see http://omronfs.omron.com/en_US/ecb/products/pdf/en-a6s.pdf)")
	(tags "SMD DIP Switch SPST Slide 8.9mm 350mil")
	(property "Reference" "REF**"
		(at 0 -12.96 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIP_SPSTx09_Slide_Omron_A6S-910x_W8.9mm_P2.54mm"
		(at 0 12.96 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 2.3 0 90)
		(layer "F.Fab")
	)
	(fp_text user "on"
		(at 0.075 -11.305 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.45 -10.16)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "2" smd roundrect
		(at -4.45 -7.62)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "3" smd roundrect
		(at -4.45 -5.08)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "4" smd roundrect
		(at -4.45 -2.54)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "5" smd roundrect
		(at -4.45 0)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "6" smd roundrect
		(at -4.45 2.54)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "7" smd roundrect
		(at -4.45 5.08)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "8" smd roundrect
		(at -4.45 7.62)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "9" smd roundrect
		(at -4.45 10.16)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "10" smd roundrect
		(at 4.45 10.16)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "11" smd roundrect
		(at 4.45 7.62)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "12" smd roundrect
		(at 4.45 5.08)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "13" smd roundrect
		(at 4.45 2.54)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "14" smd roundrect
		(at 4.45 0)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "15" smd roundrect
		(at 4.45 -2.54)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "16" smd roundrect
		(at 4.45 -5.08)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "17" smd roundrect
		(at 4.45 -7.62)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "18" smd roundrect
		(at 4.45 -10.16)
		(size 1.5 1.1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx09_Slide_Omron_A6S-910x_W8.9mm_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
