(footprint "SW_DIP_SPSTx10_Slide_9.78x27.58mm_W8.61mm_P2.54mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SMD 10x-dip-switch SPST , Slide, row spacing 8.61 mm (338 mils), body size 9.78x27.58mm (see e.g. https://www.ctscorp.com/wp-content/uploads/204.pdf), SMD")
	(tags "SMD DIP Switch SPST Slide 8.61mm 338mil SMD")
	(property "Reference" "REF**"
		(at 0 -14.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_DIP_SPSTx10_Slide_9.78x27.58mm_W8.61mm_P2.54mm"
		(at 0 14.85 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 3.46 0 90)
		(layer "F.Fab")
	)
	(fp_text user "on"
		(at 1.3075 -12.9275 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.305 -11.43)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "2" smd roundrect
		(at -4.305 -8.89)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "3" smd roundrect
		(at -4.305 -6.35)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "4" smd roundrect
		(at -4.305 -3.81)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "5" smd roundrect
		(at -4.305 -1.27)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "6" smd roundrect
		(at -4.305 1.27)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "7" smd roundrect
		(at -4.305 3.81)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "8" smd roundrect
		(at -4.305 6.35)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "9" smd roundrect
		(at -4.305 8.89)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "10" smd roundrect
		(at -4.305 11.43)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "11" smd roundrect
		(at 4.305 11.43)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "12" smd roundrect
		(at 4.305 8.89)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "13" smd roundrect
		(at 4.305 6.35)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "14" smd roundrect
		(at 4.305 3.81)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "15" smd roundrect
		(at 4.305 1.27)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "16" smd roundrect
		(at 4.305 -1.27)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "17" smd roundrect
		(at 4.305 -3.81)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "18" smd roundrect
		(at 4.305 -6.35)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "19" smd roundrect
		(at 4.305 -8.89)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(pad "20" smd roundrect
		(at 4.305 -11.43)
		(size 2.44 1.12)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.223214)
	)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_DIP_SPSTx10_Slide_9.78x27.58mm_W8.61mm_P2.54mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
)
