(footprint "SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)")
	(tags "push horizontal SPST 1P1T")
	(property "Reference" "REF**"
		(at 0 -2.7 180)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
		(at 0 2.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.125 0)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.125 0)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.225 -0.9)
		(size 0.75 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at 1.225 -0.9)
		(size 0.75 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0 -0.9)
		(size 0.6 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -1.85 1.05)
		(size 1.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 1.85 1.05)
		(size 1.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
