(footprint "SW_Push_1P1T-SH_NO_CK_KMR2xxG"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CK components KMR2 tactile switch with ground pin http://www.ckswitches.com/media/1479/kmr2.pdf")
	(tags "tactile switch kmr2")
	(property "Reference" "REF**"
		(at 0 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Push_1P1T-SH_NO_CK_KMR2xxG"
		(at 0 2.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.45 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0 -1.425)
		(size 1.7 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-SH_NO_CK_KMR2xxG.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
