(footprint "SW_Push_1P1T_NO_CK_PTS125Sx43PSMTR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C&K Switches 1P1T SMD PTS125 Series 12mm Tact Switch with Pegs, https://www.ckswitches.com/media/1462/pts125.pdf")
	(tags "Button Tactile Switch SPST 1P1T")
	(property "Reference" "REF**"
		(at 0 -7.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Push_1P1T_NO_CK_PTS125Sx43PSMTR"
		(at 0 7.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -4.5)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 4.5)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -7.15 -2.5)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 7.15 -2.5)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -7.15 2.5)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 7.15 2.5)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_CK_PTS125Sx43PSMTR.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
