(footprint "SW_Push_1P1T_XKB_TS-1187A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Tactile Switch, http://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf")
	(tags "SPST Tactile Switch")
	(property "Reference" "REF**"
		(at 0 -3.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Push_1P1T_XKB_TS-1187A"
		(at 0 3.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3.75 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3 -1.875)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 3 -1.875)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3 1.875)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3 1.875)
		(size 1 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_XKB_TS-1187A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
