(footprint "SW_Push_1TS009xxxx-xxxx-xxxx_6x6x5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "tactile push button, 6x6mm, height=5mm, 12V 50mA, https://datasheet.lcsc.com/lcsc/1811151231_HYP--Hongyuan-Precision-1TS009A-1800-5000-CT_C319409.pdf")
	(tags "tact sw push 6mm silicone rubber")
	(property "Reference" "REF**"
		(at 0 -4.064 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Push_1TS009xxxx-xxxx-xxxx_6x6x5mm"
		(at 0 3.81 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "REF**"
		(at 0 -4.064 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.254 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3 0)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 3 0)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1TS009xxxx-xxxx-xxxx_6x6x5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
