(footprint "SW_SPDT_PCM12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SPDT_PCM12"
		(at 0 4.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3.2 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -3.65 -0.78)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at -3.65 1.43)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" np_thru_hole circle
		(at -1.5 0.33)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 1.5 0.33)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" smd rect
		(at 3.65 -0.78)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "" smd rect
		(at 3.65 1.43)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at -2.25 -1.43)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.75 -1.43)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.25 -1.43)
		(size 0.7 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPDT_PCM12.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
