(footprint "SW_SPST_CK_KMS2xxGP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Microminiature SMT Side Actuated, 4.2 x 2.8 x 1.42mm with pegs, https://www.ckswitches.com/media/1482/kms.pdf")
	(tags "Switch SPST KMS2")
	(property "Reference" "REF**"
		(at 0 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SPST_CK_KMS2xxGP"
		(at 0 3.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -0.975 0.75)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0.975 0.75)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "1" smd roundrect
		(at 2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "2" smd roundrect
		(at -2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "2" smd roundrect
		(at 2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(pad "SH" smd roundrect
		(at 0 -1.425)
		(size 1.7 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_CK_KMS2xxGP.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
