(footprint "SW_SPST_EVQP7C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Light Touch Switch, 2.2 N, https://www3.panasonic.biz/ac/e_download/control/switch/light-touch/catalog/sw_lt_eng_3529s_side.pdf?f_cd=402906")
	(tags "tactile switch")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SPST_EVQP7C"
		(at 0 3.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -2.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 -0.9)
		(size 0.7 0.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 0.9)
		(size 0.7 0.7)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.8 -0.72)
		(size 1.4 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "1" smd roundrect
		(at 1.8 -0.72)
		(size 1.4 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "2" smd roundrect
		(at -1.8 0.72)
		(size 1.4 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(pad "2" smd roundrect
		(at 1.8 0.72)
		(size 1.4 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP7C.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
