(footprint "SW_Tactile_SPST_NO_Straight_CK_PTS636Sx25SMTRLFS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tactile switch, SPST, 6.0x3.5 mm, H2.5 mm, straight, NO, gull wing leads: https://www.ckswitches.com/media/2779/pts636.pdf")
	(tags "switch tactile SPST 1P1T straight NO SMTR C&K")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Tactile_SPST_NO_Straight_CK_PTS636Sx25SMTRLFS"
		(at 0 3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.875 0)
		(size 1.25 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.875 0)
		(size 1.25 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Tactile_SPST_NO_Straight_CK_PTS636Sx25SMTRLFS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
