(footprint "SW_MEC_5GTH9"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MEC 5G single pole normally-open tactile switch https://cdn.sos.sk/productdata/80/f6/aabf7be6/5gth9358222.pdf")
	(tags "switch normally-open pushbutton push-button")
	(property "Reference" "REF**"
		(at 0.475 -1.85 180)
		(layer "F.SilkS")
	)
	(property "Value" "SW_MEC_5GTH9"
		(at 3.8 13 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.76 5.03 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 10.16 90)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 0 90)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.62 10.16 90)
		(size 1.8 1.8)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_MEC_5GTH9.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
