(footprint "SW_PUSH_1P1T_6x3.5mm_H4.3_APEM_MJTP1243"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "tactile push button, 6x3.5mm, https://www.apem.com/idec-apem/en_US/PCB-switches/Tactile-Switches/MJTP-6mm-through-hole/c/MJTP_6mm_through%20hole?page=1")
	(tags "PHAP3362 6mm tact sw THT")
	(property "Reference" "REF**"
		(at 3.42 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_PUSH_1P1T_6x3.5mm_H4.3_APEM_MJTP1243"
		(at 4.4 3.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 2.25 2.25)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.5 0 90)
		(size 2.25 2.25)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_1P1T_6x3.5mm_H4.3_APEM_MJTP1243.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
