(footprint "SW_SPST_Omron_B3F-40xx"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SW_THT_Tactile_Omron_B3F-40xx, 12x12 mm, Through hole switch from the B3F Family manufactured by Omron,  https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
	(tags "tactile switch THT button push B3F-4000 B3F-4050 B3F-4005 B3F-4055  ")
	(property "Reference" "REF**"
		(at 6.25 -5.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SPST_Omron_B3F-40xx"
		(at 6.25 10.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 6.25 2.5 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 6.25 -2)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.25 7)
		(size 1.8 1.8)
		(drill 1.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 2.9 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole oval
		(at 12.5 0)
		(size 2.9 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 5)
		(size 2.9 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 12.5 5)
		(size 2.9 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_SPST_Omron_B3F-40xx.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
