(footprint "SW_Tactile_SPST_Angled_PTS645Vx58-2LFS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "tactile switch SPST right angle, PTS645VL58-2 LFS")
	(tags "tactile switch SPST angled PTS645VL58-2 LFS C&K Button")
	(property "Reference" "REF**"
		(at 2.25 1.68 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_Tactile_SPST_Angled_PTS645Vx58-2LFS"
		(at 2.25 5.38988 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.25 1.68 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -1.25 2.49)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" thru_hole circle
		(at 5.76 2.49)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.75 1.75)
		(drill 0.99)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 4.5 0)
		(size 1.75 1.75)
		(drill 0.99)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx58-2LFS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
