(footprint "Buzzer_Mallory_AST1240MLQ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Mallory low-profile piezo buzzer, https://www.mspindy.com/specifications/AST12140MLQ.pdf")
	(tags "piezo buzzer")
	(property "Reference" "REF**"
		(at 0 -7.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Buzzer_Mallory_AST1240MLQ"
		(at 0 7.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Sound Exit Hole"
		(at 0 -5 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6 0)
		(size 3 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 6 0)
		(size 3 6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_Mallory_AST1240MLQ.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
