(footprint "Indicator_PUI_AI-1440-TWT-24V-2-R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14mm Indicator, https://www.puiaudio.com/media/SpecSheet/AI-1440-TWT-24V-2-R.pdf")
	(tags "piezo buzzer self drive oscillator")
	(property "Reference" "REF**"
		(at 3.8 -8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Indicator_PUI_AI-1440-TWT-24V-2-R"
		(at 3.8 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.8 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.147)
	)
	(pad "2" thru_hole circle
		(at 7.6 0)
		(size 1.7 1.7)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Indicator_PUI_AI-1440-TWT-24V-2-R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
