(footprint "MagneticBuzzer_PUI_SMT-1028-T-2-R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Buzzer, 2830Hz, 3.6Vpp, 90dbA@10cm, Top sound port, 10x10x3,5mm, https://api.puiaudio.com/file/612539d9-c50b-48de-88aa-b63ef8817a91.pdf")
	(tags "SMT 1028")
	(property "Reference" "REF**"
		(at 0.2 -5.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "MagneticBuzzer_PUI_SMT-1028-T-2-R"
		(at 0.1 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.1 0.1 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at -3.35 -2.95 270)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.9 -2.9 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at 4.9 -2.9 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "MP" smd roundrect
		(at -4.9 3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "MP" smd roundrect
		(at 4.9 3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/MagneticBuzzer_PUI_SMT-1028-T-2-R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
