(footprint "MagneticBuzzer_ProSignal_ABI-009-RC"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Buzzer, Elektromagnetic Beeper, Summer, 6V-DC,")
	(tags "Pro Signal ABI-009-RC ")
	(property "Reference" "REF**"
		(at 3.8 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "MagneticBuzzer_ProSignal_ABI-009-RC"
		(at 3.8 7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 3.8 -7 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at 0 -1.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 7.6 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/MagneticBuzzer_ProSignal_ABI-009-RC.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
