(footprint "PUIAudio_SMT_0825_S_4_R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD 8540, http://www.puiaudio.com/product-detail.aspx?partnumber=SMT-0825-S-4-R")
	(tags "SMD 8540")
	(property "Reference" "REF**"
		(at 0.2 -5.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "PUIAudio_SMT_0825_S_4_R"
		(at 0.1 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "+"
		(at -1.5 -3.25 270)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.1 0.1 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at -2.75 -2.75 270)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.5 -3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.5 3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 3.5 3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 3.5 -3.5 270)
		(size 2 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/PUIAudio_SMT_0825_S_4_R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
