(footprint "Speaker_CUI_CMR-1206S-67"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Speaker, 30mW, 300-7000Hz, IP67 face, 12x6x2,25mm, https://www.cuidevices.com/product/resource/cmr-12062s-67.pdf")
	(tags "speaker CUI")
	(property "Reference" "REF**"
		(at 0 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Speaker_CUI_CMR-1206S-67"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.4 2.3 180)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at 5.4 2.3 180)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Speaker_CUI_CMR-1206S-67.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
