(footprint "CP_Elec_CAP-XX_DMF3Zxxxxxxxx3D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "5.5V, 470mF supercapacitor, 45mohm, -40ºC to +70ºC, https://www.cap-xx.com/wp-content/uploads/datasheets/CAP-XX-DMF470mF-Datasheet.pdf")
	(tags "supercap")
	(property "Reference" "REF**"
		(at -8.75 -7.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "CP_Elec_CAP-XX_DMF3Zxxxxxxxx3D"
		(at 0.35 8.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -14 -3.5 180)
		(size 4 2.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -14 0 180)
		(size 4 2.5)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at -14 3.5 180)
		(size 4 2.5)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_CAP-XX_DMF3Zxxxxxxxx3D.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
