(footprint "C_1812_4532Metric_Pad1.57x3.40mm_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor handsolder")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_1812_4532Metric_Pad1.57x3.40mm_HandSolder"
		(at 0 2.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.1375 0)
		(size 1.575 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15873)
	)
	(pad "2" smd roundrect
		(at 2.1375 0)
		(size 1.575 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15873)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
