(footprint "C_Axial_L17.0mm_D7.0mm_P20.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C, Axial series, Axial, Horizontal, pin pitch=20mm, , length*diameter=17*7.0mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
	(tags "C Axial series Axial Horizontal pin pitch 20mm  length 17mm diameter 7.0mm")
	(property "Reference" "REF**"
		(at 10 -4.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_Axial_L17.0mm_D7.0mm_P20.00mm_Horizontal"
		(at 10 4.62 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 20 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L17.0mm_D7.0mm_P20.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
