(footprint "C_Radial_D6.3mm_H5.0mm_P2.50mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C, Radial series, Radial, pin pitch=2.50mm, diameter=6.3mm, height=5mm, Non-Polar Electrolytic Capacitor")
	(tags "C Radial series Radial pin pitch 2.50mm diameter 6.3mm height 5mm Non-Polar Electrolytic Capacitor")
	(property "Reference" "REF**"
		(at 1.25 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_Radial_D6.3mm_H5.0mm_P2.50mm"
		(at 1.25 4.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.25 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D6.3mm_H5.0mm_P2.50mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
