(footprint "C_Rect_L4.6mm_W3.0mm_P2.50mm_MKS02_FKP02"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*3.0mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
	(tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 3.0mm Capacitor")
	(property "Reference" "REF**"
		(at 1.25 -2.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_Rect_L4.6mm_W3.0mm_P2.50mm_MKS02_FKP02"
		(at 1.25 2.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 1.25 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.4 1.4)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W3.0mm_P2.50mm_MKS02_FKP02.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
