(footprint "CP_EIA-1608-08_AVX-J_Pad1.25x1.05mm_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tantalum Capacitor SMD AVX-J (1608-08 Metric), IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/48064/_t58_vmn_pt0471_1601.pdf), generated with kicad-footprint-generator")
	(tags "capacitor tantalum")
	(property "Reference" "REF**"
		(at 0 -1.48 0)
		(layer "F.SilkS")
	)
	(property "Value" "CP_EIA-1608-08_AVX-J_Pad1.25x1.05mm_HandSolder"
		(at 0 1.48 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.8 0)
		(size 1.25 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(pad "2" smd roundrect
		(at 0.8 0)
		(size 1.25 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.238095)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-1608-08_AVX-J.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
