(footprint "CP_EIA-7260-38_AVX-R_Pad2.68x6.30mm_HandSolder"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tantalum Capacitor SMD AVX-R (7260-38 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator")
	(tags "capacitor tantalum")
	(property "Reference" "REF**"
		(at 0 -4.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "CP_EIA-7260-38_AVX-R_Pad2.68x6.30mm_HandSolder"
		(at 0 4.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.9375 0)
		(size 2.675 6.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.093458)
	)
	(pad "2" smd roundrect
		(at 2.9375 0)
		(size 2.675 6.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.093458)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7260-38_AVX-R.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
