(footprint "DTF13-12Px"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.te.com/usa-en/product-DTF13-12PA-G003.html")
	(tags "DEUTSCH DT header 12 pin ")
	(property "Reference" "REF**"
		(at 12.192 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "DTF13-12Px"
		(at 11.6 23.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.7 18.9 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -6.0325 2.2098)
		(size 2.4 2.4)
		(drill 2.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 28.2575 2.2098)
		(size 2.4 2.4)
		(drill 2.4)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 4.445 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 8.89 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 13.335 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 17.78 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 22.225 0)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 22.225 4.445)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 17.78 4.445)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 13.335 4.445)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 8.89 4.445)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 4.445 4.445)
		(size 3 3)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 0 4.445)
		(size 3.556 3.556)
		(drill 1.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/DTF13-12Px.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
