(footprint "FanPinHeader_1x03_P2.54mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
	(tags "pin header 3-pin CPU fan")
	(property "Reference" "REF**"
		(at 2.5 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "FanPinHeader_1x03_P2.54mm_Vertical"
		(at 2.55 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.45 1.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 90)
		(size 2.03 1.73)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 2.54 0 90)
		(size 2.03 1.73)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 5.08 0 90)
		(size 2.03 1.73)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
