(footprint "IHI_B6A-PCB-45_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://lugsdirect.com/PDF_Webprint/B6A-PCB-45-XX(-X).pdf")
	(tags "connector IHI B6A-PCB-45")
	(property "Reference" "REF**"
		(at 0.05 -5.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "IHI_B6A-PCB-45_Vertical"
		(at 0 -0.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 -5.75 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -6.05 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -6.05 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -4.45 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.85 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.25 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.35 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 -3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 -2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 -1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 -0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 0.55 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 1.65 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 2.75 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 4.78 3.85 180)
		(size 1.3 0.8)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at 0 0 180)
		(size 14.7 9.8)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/IHI_B6A-PCB-45_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
