(footprint "Joint-Tech_C5080WR-04P_1x04_P5.08mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C5080 SERIES 90° Wafer, (https://datasheet.lcsc.com/lcsc/1912261836_HR-Joint-Tech-Elec-C5080WR-04P_C477015.pdf)")
	(tags "connector side-entry ATA PATA IDE 5.25 inch floppy drive power")
	(property "Reference" "REF**"
		(at 7.62 -2.55 180)
		(layer "F.SilkS")
	)
	(property "Value" "Joint-Tech_C5080WR-04P_1x04_P5.08mm_Vertical"
		(at 7.62 11.45 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 5.45 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 2.6 2.55)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0 180)
		(size 2.6 2.6)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0 180)
		(size 2.6 2.6)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 15.24 0 180)
		(size 2.6 2.6)
		(drill 1.52)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -4.38 5.45 180)
		(size 4 4)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 19.62 5.45 180)
		(size 4 4)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/Joint-Tech_C5080WR-04P_1x04_P5.08mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
